**Crop Residue Management**

**Application Rates/Methods:**

***Initial treatment:***

Apply 1 to 2 qts. per acre following harvest.

***Treatment may vary due to residue load.***

***Mix 1 gallon of Waste Away® per 10 gallons of water.***